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STATE LIFE INSURANCE CORPORATION OF PAKISTAN

SHEIKHUPURAZONE 

TENDER NOTICE # HRA&P /SKP/ 02/ 2026 (CCTV IP CAMERA’S)
State life Insurance Corporation of Pakistan, invites Bids in accordance with PPRA rules, under Single Stage- Two Envelops procedure from experienced & reputed GST/Income Tax/Sales Tax Registered Firms/Dealer/Supplier (Federal/Provincial) having relevant experience for Procurement CCTV IP Cameras alongwith NVR’s and LCD’s for its State Life Zonal Office, Al-Sharif Plaza, Near Children Hospital, Sargodha Road, Sheikhupura through E-PADS (2.0V) through https://epads.gov.pk/ 
	Title of Works
	Qty
	Estimated Cost
	Closing date & time for Submission of Bids
	Date & Time of Opening of Technical Bids

	CCTV IP CAMERAS
I 4MP Entry IR Fixed-Focal Bullet Network Camera,   4MP, 1/3” CMOS image sensor, low luminance, high image definition, Outputs max. 4MP (1920 × 1080) @25/30 fps, H.265 codec, high compression rate, ultra-low bit rate, Built-in efficient IR illuminator, and the max. illumination IR distance: 30 m, ROI, SMART H.264/H.265+, flexible coding, applicable to various bandwidth                   and storage environments, Rotation mode, DWDR, 3D NR, HLC, BLC, digital watermarking, applicable  to various monitoring scenes, Abnormality detection: Motion detection, video tampering, network  disconnection, IP conflict, illegal access, 12V DC/PoE power support, IP67 protection. 
I. II  32 Channel 10 2HDDs Network video Recorder, New 4.0 user interface, security baseline 2.1.H.264, h.265, Smart H.264+, and Smart H.265+, H.265auto switch. Max. Decoding capability: 8 x 1080p@30 fps. Supports adaptive adaptive decoding. Supports mainstream cameras of ONVIF and RTSP protocols. P2P remote surveillance, video play on mobile device. VGA/HDMI simultaneous video output, maximum resolution of HDMI is 4K. Al by Camera: Face detection, perimeter protection, IVS, people counting, heat map and SMD. Supports remote configuration and management of IPC, such as set ting parameters, getting information and upgrading IPC of the same model in batches 2 SATA 111 ports, upto 10 TB for a single HDD. The maximum HDD capacity varies with environment temperature

II. III  16 Channel 10 2HDDs Network video Recorder, New 4.0 user interface, security baseline 2.1.H.264, h.265, Smart H.264+, and Smart H.265+, H.265auto switch. Max. Decoding capability:8 x 1080p

 @ 30 fps. Supports adaptive adaptive decoding. Supports mainstream cameras of ONVIF and RTSP protocols. P2P remote surveillance, video play on mobile device. VGA/HDMI simultaneous video output, maximum resolution of HDMI is 4K. Al by Camera: Face detection, perimeter protection, IVS, people counting, heat map and SMD. Supports remote configuration and management of IPC, such as set ting parameters, getting information and upgrading IPC of the same model in batches 2 SATA 111 ports, upto 10 TB for a single HDD. The maximum HDD capacity varies with environment temperature

IV  Surveillance 8TB
V   Surveillance 4TB
VI   LED 40’’ (HD)

VII  LED 32’’ (HD)
I. Complete Installation and Commissioning is the responsibility of the vendor with the following required material on turnkey basis. 
· PoE Switch 08/16 Port, Cat6 Cable 23AWG, PVC Box, Data Rack 1U, RJ-45 Connectors and tagging of each camera point, Duct 16x25, 16x38, 40x40, Pipe 1”,1.5”,2” Power Cable 40/76, Flexible Pipe 1”, 02 Core Single Mode Fiber Cable, Media Converter, Splicing etc.
Special Note; 

· Vendors Site Survey must be conducted at our location State Life Insurance Lahore Sargodha Road, Near Children Hospital, Sheikhupura for actual measurement of the above items for Cameras point and NVR & 3 LED place/location as per Diagram (3 pages) attached. 
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	2,050,000/-


	22.10.2026 Until 

10:00 a.m.
	22.10.2026               at

10:30 a.m.




Signature & Seal (by vendor)

